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Circuit for the efficient production of Heat
3 2-/5-09

using an inductive resistor heating element and the
recapture and recycling of the inductive collapse




